[Version]
Signature=$CHICAGO$
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318}
Provider=%WW%
DriverVer = 01/01/2002,1.15.0.0 
;CatalogFile = KS-959.cat

[DestinationDirs]
DefaultDestDir=11
KS959_CopyFiles=11
;KS959_CopyInfFiles=17

[Manufacturer]
%WW%=MA_Devices

[ControlFlags]
ExcludeFromSelect = USB\VID_07D0&PID_4959

[MA_Devices]
%StandardExpl%=KS959_Install,USB\VID_07D0&PID_4959

[SourceDisksNames]
1="KS-959 Software CD",,,

[KS959_Install]
DeviceID=,USB\VID_07D0&PID_4959
CopyFiles=KS959_CopyFiles, KS959_CopyInfFiles
AddReg=KS959_AddReg, KS959.reg
MaxInstance=1

[KS959_AddReg]
;
;  This section describes additions to the Windows registry.
;  See the Windows 95 Resource kit and be sure of what you're
;  doing before making changes.  You can use the regedit.exe tool that
;  comes with Windows 95/NT to browse the registry.
;
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,KS-959.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

;
; NDIS Info
;
HKR,NDIS,LogDriverName,,"KS-959"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
; Interfaces
HKR,NDI\Interfaces,DefUpper,0,%UpperInterface%
HKR,NDI\Interfaces,UpperRange,0,%UpperInterface%
HKR,Ndi,NetType,,1
HKR,Ndi,DeviceID,,"KS-959"
HKR,,CardType,,"PNP"

;
; NDI Registry Entry
;
HKR,Ndi,MaxInstance,,0  ;prevent multiple bindings
HKR,Ndi,NdiInstaller,,"ir_ndi.dll,IRWDM_NdiProc"
HKR,Ndi\Compatibility,RequireAll,,"IRDA"
HKR,Ndi,AdapterType,,"IrDA Infrared Miniport"
HKR,,DriverDesc,0,%StandardExpl%
HKR,NDI,HelpText,0,%KS959_HELP%

;HKR,,AdapterName,0,USB\VID_07D0&PID_4959
;HKR,Ndi\Install,,0,USB\VID_07D0&PID_4959

[KS959.reg]
HKR,Ndi\params\MaxConnectList,ParamDesc,,%MaxConnectRate%
HKR,Ndi\params\MaxConnectList,flag,1,20,00,00,00
HKR,Ndi\params\MaxConnectList,default,,"57600"
HKR,Ndi\params\MaxConnectList,type,,enum
HKR,Ndi\params\MaxConnectList\enum,"115200",,"115200"
HKR,Ndi\params\MaxConnectList\enum,"57600",," 57600"
HKR,Ndi\params\MaxConnectList\enum,"38400",," 38400"
HKR,Ndi\params\MaxConnectList\enum,"19200",," 19200"
HKR,Ndi\params\MaxConnectList\enum,"9600",,"  9600"
;HKR,Ndi\params\InfraredTransceiverType,ParamDesc,,%InfraredTransceiver%
;HKR,Ndi\params\InfraredTransceiverType,flag,1,20,00,00,00
;HKR,Ndi\params\InfraredTransceiverType,default,,0
;HKR,Ndi\params\InfraredTransceiverType,type,,enum
;HKR,Ndi\params\InfraredTransceiverType\enum,"1",,"KS-959 USB Infrared Adapter"

[KS959_CopyFiles]
KS-959.sys

[Strings]
KS959_HELP="This NDIS miniport driver installs as a network adapter and binds to the Fast IR protocol."
UpperInterface="ndisirda"
V_CLASSNAME="Network adapters"
WW="Kingsun Technology Inc."
SerialPort="Serial Port"
InfraredTransceiver="Infrared Transceiver"
StandardExpl = "KS-959 USB Infrared Adapter"
MaxConnectRate="Maxiumum Connect Rate"
